CHEMIE ALLIANCE SDN BHD
DETERMINATION OF CLOUD POINT
1.0 Apparatus
For the purpose of the determination, the following apparatus are required:

a) Beakers, 100mL capacity;

b) Ice-bath;

c) Glass rod

d) Thermometer and

e) Spatula

2.0 Procedure
a) Scope the sample into the beaker gently with spatula and fill in the sample about 1/3 height of the beaker. (Avoid not generating more bubble while filling). 

b) Make sure the sample in the beaker is clear enough not to block the vision. 

c) After that, put the beaker inside the ice-bath and stir gently the sample once a while with glass rod to make sure the temperature is equally spread. 

d) Quickly get the temperature of the sample once the sample starts to look a bit cloudy or not as clear as before. (This is cloud point of the sample).

3.0 Result
Report the cloud point of the sample in oC unit.
