Stability Study Program

The finish samples are stored at 25oC and 45oC for stability test for a period of three month. Check the Appearance, color, odour, pH and viscosity of the products from time to time to make sure the products all fall within the specification.

Batch Number System

The batch number is coded according to YY/MM/Running number. 

For example:

Batch Number: 0907001

       Year 2009    July        001 is the running number

The second batch will be: 0907002

